SPECIFICATION SHEET: WALL SCONCES, GYPSET CARGO.

**THESE ITEMS MUST BE WIRED AND INSTALLED BY A LICENCED ELECTRICIAN.**

**LAMPHOLDERS: (THEY ARE IN TWO PARTS BELOW 723.1 AND 00172 BUT CLICK TOGETHER)**

**(Supplied by Gypset Cargo)**

**Type 723.1TYPEMPHOLDER E 14**

**Plastic-lampholder E 14, one-piece**

**with snap-in fixing, smooth casing**

**and screwless pillar-connection**

Casing : PET

Resistance to leakage current : also available in PTI 250

Distance : 21 mm

Fixing by screws is also possible.

Accessories:

Snap-in caps

**Type 00172SNAP-IN CAP for lampholders E 14**

**Snap-in cap for plastic-lampholders E 14**

Material : glass-fibre reinforced polyamide

Thread : M 10 x 1

Round hole : Ø 10,2 mm

Profile hole : Ø 10,2 mm x 8,6 mm

Snap-in cap for one-piece plastic-lampholders no. 10722..... and 10723.....

Available via:

Lighting Australia

<http://www.lightingaustralia.com.au/>

**CABLE FOR ARMS**: TWO CORE PVC Double Insulated .75mm FLAT Flex. **(supplied by electrician)**

Available via:

Beal Pritchett

<http://www.bealpritchett.com.au/>