SPECIFICATION SHEET: SOPHIA GLASS LANTERN, GYPSET CARGO.

**THESE ITEMS MUST BE WIRED AND INSTALLED BY A LICENCED ELECTRICIAN.**

**LAMPHOLDERS:**

**E 14**

**Plastic-lampholder E 27, one-piece**

**Thermoplastic lampholder**

Accessories:

Dome and Shade Ring

Available via:

Lighting Australia

<http://www.lightingaustralia.com.au/>

**CABLE FOR ARMS**: TWO CORE PVC Double Insulated .75mm FLAT/ROUND Flex.

Available via:

Beal Pritchett

<http://www.bealpritchett.com.au/>

**CABLE TO CEILING**: THREE CORE Flex CABLE TO CEILING.

Flexible cord and Cable – Multi Core Ordinary Duty 250/440V PVC V90 copper conductor Flexible Cable.

Available via:

Electra Cables

<http://www.electracables.com.au/>